{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Datenblatt"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":2,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Datenblatt","index":0,"n_rows":141,"n_cols":18,"rows_kept":141,"cut":false,"hidden":false,"merged":[[138,1,138,2],[5,1,5,2],[20,1,20,2],[122,1,122,2],[118,1,118,2],[113,1,113,2],[108,1,108,2],[90,1,90,2],[84,1,84,2],[67,1,67,2],[38,1,38,2],[34,1,34,2]]}
[1000,"VTFZ","Name:",null,null,null,null,"Zulassungsart","Interoperabilitätskennzeichnung","oberer Bereich Fahrzeugumgrenzung","SIFA","Bauart MG","Bremsklotz","Antriebsart","SFZ Art","Mittelkupplung WE","ZE System","WC"]
[1000,null,"Firma / Funktion:"]
[1000,null,"Emailadresse:",null,null,null,null,"Probefahrtszulassung","RIV","G1","Vorhanden Typ unbekannt","Hochlage","GG","derzeit nicht bekannt","KL Z","Standardpuffer",1,"offen"]
[1000,null,"Datum:",null,null,null,null,"inländische IBG","RIC","G2","Weg-Weg","Tieflage","LL","Diesel-Elektrisch","KL X","Diagonalpuffer",1.2,"geschlossen"]
[0,null,null,null,null,null,null,"ausländische IBG","TEN","GA","Weg-Zeit",null,"K","Diesel-Hydrodynamisch","SKL X","Kuppelstange",1.5]
[0,"ALLGEMEINE ANGABEN",null,"Fahrzeugdaten","Einheit","Beispiel",null,null,"GE","GB","Zeit-Weg",null,null,"Diesel-Hydrostatisch","SKL Z","Sonderbauart"]
[3,"1.1","TSI-Fahrzeugnummer (12-stellig)",null,null,"9281 2016 922-4",null,null,"TEN RIV","GC","Zeit-Zeit",null,null,"Elektrisch"]
[9,"1.3","alternative Fahrzeugbezeichnung",null,null,"2016 922",null,null,null,"DE2"]
[13,"1.4","Halter",null,null,"LTE Logistik- und Transport GmbH"]
[12,"1.5","VKM (Fahrzeughalterkennung / Vehicle Keeper Marking)",null,null,"LTE"]
[32,"1.6","früheres VKM",null,null,"ggf. vorheriges VKM eintragen (z.B. DISPO)"]
[14,"1.9","für die Instandhaltung verantwortliche Stelle (ECM)",null,null,"LTE Logistik- und Transport GmbH"]
[17,"1.10","Zulassungsart",null,null,"lt. Auswahlliste (z.B. inländische IBG)"]
[18,"1.11","Betriebsbewilligung / Inbetriebnahmegenehmigung Behörde",null,null,"BMVIT 350.922/0001-II/Sch4/2005  vom  …"]
[33,"1.13","Vermieter",null,null,"LTE Logistik- und Transport GmbH"]
[24,"1.14","Bedingungen für Zugeinreihung",null,null,"keine"]
[25,"1.15","Nachschiebeverbot",null,null,"Nein"]
[26,"1.16","maximale betrieblich ertragbare Längsdruckkraft (LDK)",null,"kN","max. betriebl. kN-Wert eintragen falls < 240kN "]
[28,"1.17","Anmerkungen"]
[0]
[0,"GRUNDDATEN",null,"Fahrzeugdaten","Einheit","Beispiel"]
[34,"2.1","Erzeuger (Hersteller)",null,null,"Siemens AG"]
[35,"2.2","Herstellerbezeichnung des Fahrzeuges",null,null,"EuroRunner"]
[41,"2.3","Typenbezeichnung",null,null,"ER20"]
[42,"2.4","Variante",null,null,"V2"]
[43,"2.5","Baujahr",null,null,2004]
[44,"2.6","Umbaujahr (der letzten Veränderung des Fahrzeuges)",null,null,"Umbaujahr eintragen (z.B. Variantenänderung, …)"]
[36,"2.7","Fabrikationsnummer (Maschinennummer)",null,null,21030]
[37,"2.8","eindeutige Kennnummer",null,null,"ggf. als Ergänzung zur Fabrikationsnr. eintragen"]
[38,"2.9","erste Funk GSM-R CT3-Nummer",null,null,"3 02016922 01  (CT3 + 8-stellig + FC)"]
[45,"2.11","erste Funk GSM-R CT4-Nummer",null,null,"4 xxxxxxxxx 01  (CT4 + 9-stellig + FC)"]
[40,"2.13","Fahrzeug-Software (Version)",null,null,"Release K_FMZ"]
[47,"2.14","Fahrzeug-Software (Stand vom)",null,null,"2012-02-15"]
[0]
[0,"ZULASSUNGSDATEN",null,"Fahrzeugdaten","Einheit","Beispiel"]
[48,"3.1","Mitgliedsstaat Register",null,null,"Österreich, Deutschland, …"]
[51,"3.8","Instandhaltungsregelwerk",null,null,"ggf. eintragen"]
[0]
[0,"BETRIEBLICHE DATEN",null,"Fahrzeugdaten","Einheit","Beispiel"]
[85,"4.1","Spurweite",null,"mm",1435]
[86,"4.2","IBE Bewertungsziffer",null,null,"0,931 (Berechnung lt. Anforderungskatalog TFZ)"]
[88,"4.3","Achsanzahl",null,null,4]
[89,"4.4","Achsfolge",null,null,"Bo´Bo´"]
[59,"4.5","Vmax mit Eigenantrieb",null,"km/h",140]
[60,"4.6","Vmax geschleppt",null,"km/h",140]
[61,"4.7","Vmax unter bestimmten Bedingungen",null,"km/h","ggf. eintragen (z.B. richtungsabhängige Vmax, …) "]
[62,"4.8","Bedingungen für bedingte vmax",null,null,"zu Pkt. 4.7 gehörige Bedingungen "]
[63,"4.9","maximale nicht ausgeglichene Querbeschleunigung",null,"m/s2",1]
[65,"4.11","Länge über Puffer / Gesamtlänge",null,"mm",19275]
[66,"4.12","maximaler Abstand letzter Radsatz Fahrzeugende",null,"mm",3107]
[67,"4.13","Achsabstand / Drehzapfenabstand",null,"mm",10362]
[68,"4.14","Drehgestell-Ax-Abstand - iDG",null,"mm",2700]
[69,"4.15","maximaler Abstand von zwei Radsätzen - iR",null,"mm",7662]
[90,"4.16","minimal befahrbarer Kuppenradius",null,"m",250]
[91,"4.17","minimal befahrbarer Wannenradius",null,"m",300]
[70,"4.23","oberer Bereich Fahrzeugumgrenzung",null,null,"lt. Auswahlliste (z.B. G1 [gemäß UIC 505-1])"]
[71,"4.24","Bemerkung zum oberen Bereich der Fahrzeugumgrenzung",null,null,"ggf. eintragen"]
[72,"4.25","Profil unten für Gleisbremsen geeignet",null,null,"Nein"]
[74,"4.27","minimaler Bogenhalbmesser im Zug",null,"m",100]
[76,"4.28","minimaler Bogenhalbmesser als Einzelfahrzeug bzw. in langgemachtem Zustand",null,"m","ggf. eintragen"]
[77,"4.30","minimaler Bogenhalbmesser unter bestimmten  Bedingungen",null,"m",80]
[78,"4.31","Bedingungen für den oben genannten Bogenradius",null,null,"Werkstättengleise, Abstellanlagen, …"]
[97,"4.32","maximale Radsatzlast",null,"t",20]
[101,"4.36","Streckenklasse des Fahrzeuges nach EN15528",null,null,"C2"]
[79,"4.51","NBÜ",null,null,"Ja"]
[80,"4.52","NBÜ Anmerkung",null,null,"Mehrfachauswahl möglich (NBÜ DB, NBA ROLA, …)"]
[0]
[0,"ZUGSICHERUNG",null,"Fahrzeugdaten","Einheit","Beispiel"]
[116,"5.1","SIFA (Sicherheitsfahrschaltung)",null,null,"lt. Auswahlliste (z.B. Zeit-Zeit)"]
[117,"5.2","Zugfunk (Bauart)",null,null,"Dualfunk (Gerätetyp z.B. Mesa 23)"]
[118,"5.3","Zugfunk-Ausnahmegenehmigung",null,null,"z.B.nur mobiles Funkgerät(mit GZ.d. Ausnahmegen.) "]
[119,"5.4","Registriereinrichtung",null,null,"Deuta DSK 10"]
[122,"5.5","PZB vorhanden",null,null,"Ja"]
[123,"5.6","PZB Typ",null,null,"PZB90"]
[124,"5.7","LZB vorhanden",null,null,"Ja"]
[125,"5.8","LZB Typ",null,null,"LZB80E"]
[126,"5.9","ETCS vorhanden",null,null,"Ja"]
[127,"5.10","ETCS Level",null,null,"Mehrfachauswahl möglich (Level STM, Level 2, …)"]
[128,"5.11","ETCS Version",null,null,"SRS 2.3.0d"]
[129,"5.12","ETCS ab Datum",null,null,"2014-07-02"]
[130,"5.13","ETCS Bemerkung",null,null,"Siemens Trainguard 200 (OBU-SW: CHP 03.01)"]
[120,"5.14","Ausnahmegenehmigungen für Zugbeeinflussungssysteme",null,null,"ggf. eintragen (mit GZ. d. Ausnahmegenehmigung)"]
[121,"5.15","sonstige Zugbeeinflussungssysteme",null,null,"z.B. Mirel, EVM 120, Integra, ZUB, …"]
[0]
[0,"GEWICHTE",null,"Fahrzeugdaten","Einheit","Beispiel"]
[132,"6.2","Betriebsmasse, betriebsbereites Fahrzeug (lt. EN 15663)",null,"t","80 (= Dienstgewicht mit 2/3 Vorräte)"]
[134,"6.4","Auslegungsmasse, betriebsbereites Fahrzeug (lt. EN 15663)",null,"t","82 (= max. Gesamtgewicht)"]
[137,"6.7","Reibungsgewicht",null,"t",80]
[141,"6.11","Schwerpunktshöhe betriebsbereites Fahrzeug",null,"mm",2.12]
[0]
[0,"BREMSDATEN",null,"Fahrzeugdaten","Einheit","Beispiel"]
[145,"7.1","Bremsbauart",null,null,"SW-GPR-E-mZ"]
[146,"7.2","Mg-Bremse",null,null,"Nein"]
[null,"7.3","Bauart der Mg-Bremse",null,null,"ggf. lt. Auswahlliste"]
[147,"7.4","Wirbelstrombremse",null,null,"Nein"]
[148,"7.9","Bremsgewicht R",null,"t",120]
[149,"7.10","Bremsgewicht P",null,"t",72]
[150,"7.11","Bremsgewicht G",null,"t",65]
[157,"7.12","Bremsgewicht R + E",null,"t",120]
[158,"7.13","Bremsgewicht P + E",null,"t"]
[159,"7.14","Bremsgewicht R + E 160",null,"t"]
[160,"7.15","Bremsgewicht P + E 160",null,"t"]
[161,"7.16","Bremsgewicht R + Mg",null,"t"]
[162,"7.17","Bremsgewicht P + Mg",null,"t"]
[151,"7.18","Feststellbremsgweicht",null,"t",20]
[208,"7.18a","Haltekraft der Feststellbremse",null,"kN"]
[152,"7.19","Anmerkung zur Feststellbremse",null,null,"Federspeicherbremse"]
[0]
[0,"ANTRIEB",null,"Fahrzeugdaten","Einheit","Beispiel"]
[165,"8.2","Antriebsart",null,null,"lt. Auswahlliste (z.B. Diesel-Elektrisch)"]
[164,"8.3","Antriebsleistung",null,"kW",2000]
[166,"8.4","Antrieb (Drehmomentübertragung zum Radsatz)",null,null,"z.B. Ritzelhohlwellenantrieb (RHA), Tatzlagerantrieb, …"]
[0]
[0,"LAUFWERK",null,"Fahrzeugdaten","Einheit","Beispiel"]
[169,"9.3","Radprofil",null,null,"DIN 5573E 1422-140 S1002"]
[172,"9.6","Spurkranzschmiereinrichtung",null,null,"Ja"]
[null,"9.7","Können die Räder eines Radsatzes gegenseitig isoliert werden?",null,null,"Nein"]
[0]
[0,"ELEKTRISCHE DATEN",null,"Fahrzeugdaten","Einheit","Beispiel"]
[175,"10.3","Leistungssteuerung",null,null,"z.B. GTO-Wechselrichter, Einspritzpumpe, … "]
[176,"10.4","Zugsammelschiene",null,null,"z.B: AC 1000V / 50-60Hz (max. 400kVA), keine, … "]
[0]
[0,"ALLGEMEINE, ERGÄNZENDE DATEN",null,"Fahrzeugdaten","Einheit","Beispiel"]
[178,"11.1","Zusatzeinrichtungen oder besondere Aufbauten am Fahrzeug",null,null,"ggf. eintragen"]
[194,"11.9","Stoßeinrichtung gemäß UIC bzw. EN15551",null,null,"Ja"]
[195,"11.10","Puffertellerabmessungen und -radius",null,"mm","z.B. 340x550 bzw. D500"]
[196,"11.11","Pufferhub",null,"mm","z.B. 105"]
[197,"11.12","Arbeitsaufnahmevermögen (Kategorie nach UIC bzw. EN15551)",null,"kJ","z.B. 55 , 70 , … "]
[199,"11.13","Crashpuffer",null,null,"Ja"]
[200,"11.14","Zugeinrichtungssystem gemäß EN15566\n(UIC Schraubenkupplung und Zugeinrichtung)",null,"MN","lt. Auswahlliste (z.B. 1,5)"]
[198,"11.15","Stoßeinrichtung wenn nicht UIC-Standard (bzw. EN15551)",null,null,"ggf. eintragen"]
[201,"11.16","Zugeinrichtung wenn nicht UIC-Standard (bzw. EN15556)",null,null,"ggf. eintragen"]
[202,"11.17","Rangierkupplung",null,null,"ggf. eintragen (z.B. RK 900)"]
[203,"11.18","Mittelpufferkupplung",null,null,"ggf. eintragen (z.B. AK 69e, Transpact TTK, …) "]
[204,"11.19","Bemerkung zur Mittelpufferkupplung",null,null,"ggf. eintragen"]
[205,"11.20","allgemeine Bemerkung zum Wagenende",null,null,"ggf. eintragen (UIC-Standard, …)"]
[186,"11.26","Feuerlöschsystem (Feuermelde- bzw. Feuerlöschsystem)",null,null,"z.B. Kidde Deugra (Löschmittel: Novec 1230)"]
[0]
[0,"Zusatzinformationen",null,"Fahrzeugdaten",null,"Beispiel"]
["x","\n12.1","\nsonstige Bemerkungen",null,null,"\nHier können alle Angaben eingetragen werden, welche keinem anderen Feld zugeordnet werden könnnen."]
["x","\n12.2","\nAnmerkungen ÖBB Infra AG"]